<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<description>A simple Eagle library, by David Cannings (david@edeca.net)

This is v1 and is licensed under the Creative Commons (Attribution-Non-Commercial-Share Alike 2.0 UK)

For more information, see http://edeca.net/</description>
<packages>
<package name="DIL16">
<description>Dual In Line</description>
</package>
<package name="NFM-12881BG-11">
<description>NFM-12881 Single Colour 8x8 LED Matrix

Available from

- Futurlec (LEDM88G)</description>
</package>
<package name="DC-SOCKET">
</package>
<package name="LCC8">
<description>LCC8, as used by some accelerometers</description>
</package>
<package name="UMAX8-THERMAL">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;
Source: MAX1792.pdf</description>
</package>
<package name="SPC4077-BIG-HOLES">
<description>&lt;b&gt;DC POWER JACK 2mm&lt;/b&gt;&lt;br&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1161.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
<package name="RFM12-PIN">
<description>&lt;b&gt;12 Pin - 2mm Dual Row Single Wafer, Vertical T/H HDR&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/877580616_sd.pdf</description>
</package>
<package name="TMB-6">
<description>6 lead TMB package, as used by light-to-digital converters</description>
</package>
<package name="KEYSTONE-2/3A">
<description>Keystone Electronics 2/3A battery holder</description>
</package>
<package name="SOIC28">
</package>
<package name="SSOP28">
</package>
<package name="SOT23-5">
</package>
<package name="TQFP44">
</package>
<package name="MINI-USB">
<description>Mini USB, e.g. Kyocera 24 5141 005 000 863+</description>
</package>
<package name="PINHD1X03">
</package>
<package name="PINHD1X02">
</package>
<package name="PINHD1X04">
</package>
<package name="PINHD1X05">
</package>
<package name="PINHD1X06">
</package>
<package name="PINHD1X07">
</package>
<package name="PINHD1X08">
</package>
<package name="PINHD1X08-SQUARE">
</package>
<package name="PINHD1X07-SQUARE">
</package>
<package name="PINHD1X06-SQUARE">
</package>
<package name="PINHD1X05-SQUARE">
</package>
<package name="PINHD1X04-SQUARE">
</package>
<package name="PINHD1X03-SQUARE">
</package>
<package name="PINHD1X02-SQUARE">
</package>
<package name="SO8">
</package>
<package name="DIL8">
</package>
<package name="SO20L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="KEYSTONE-CLIP-2/3A">
<description>CR123A holder

Using Keystone 92 snap-in PCB mount battery holders.</description>
</package>
<package name="KEYSTONE-CLIP-2/3AAA">
<description>A 2/3rd AAA holder made using two Keystone 82 battery clips.</description>
</package>
<package name="L1210">
<description>INDUCTOR</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN

(From microchip.lbr)</description>
</package>
<package name="SOT23">
<description>SOT23

(from diode.lbr)</description>
</package>
<package name="ROTARY-MCRM3A-10">
<description>Multicomp SMD rotary switch (e.g. MCRM3A-10R).</description>
</package>
<package name="PINHD-ICD">
<description>1x5 pin header with key markings for ICD.</description>
</package>
<package name="TYCO-USB-B-RA">
<description>TE Connectivity

USB Connector, Series B, 4 positions, R/A, SMT, with rear shell.

** NEED TO MOVE LOCKING PIN CENTRES TO CORRECT LOCATION, THEY ARE TOO NARROW **

** TODO: FIX PIN ORDER! **</description>
</package>
<package name="VISHAY-TSOP62XX">
<description>Vishay TSOP62XX, the standard IR remote control
SMD-receiver series.</description>
</package>
<package name="WURTH-744711010">
<description>Wurth 744711010 inductor (basic footprint)</description>
</package>
<package name="RJS-SW-ILLUMINATED">
<description>DPDT push switch by RJS Electronics Limited - Bedford, UK.

Previously stocked by Rapid Electronics, e.g. 78-2265.</description>
</package>
<package name="SOD-323">
<description>SOD-323 diode

Taken from Sparkfun library.</description>
</package>
<package name="QFN16">
</package>
<package name="SSOP16">
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="HTSSOP38DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf
&lt;p&gt;
(from Texas.lbr)</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
<package name="F-COAX-PCB">
</package>
<package name="PDA54-11XX">
</package>
</packages>
<symbols>
<symbol name="MIC5821">
<pin name="VCC" direction="pwr"/>
<pin name="DAT" direction="in"/>
<pin name="CLK"/>
<pin name="LAT"/>
<pin name="!OE"/>
<pin name="DOUT" direction="out"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
</symbol>
<symbol name="MIC5891">
<pin name="VCC" direction="pwr"/>
<pin name="DAT" direction="in"/>
<pin name="CLK"/>
<pin name="LAT"/>
<pin name="!OE"/>
<pin name="DOUT" direction="out"/>
<pin name="VBB" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
</symbol>
<symbol name="8X8MATRIX">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="1'" direction="out"/>
<pin name="2'" direction="out"/>
<pin name="3'" direction="out"/>
<pin name="4'" direction="out"/>
<pin name="5'" direction="out"/>
<pin name="6'" direction="out"/>
<pin name="7'" direction="out"/>
<pin name="8'" direction="out"/>
</symbol>
<symbol name="MIC5891-REV">
<pin name="VCC" direction="pwr"/>
<pin name="DAT" direction="in"/>
<pin name="CLK"/>
<pin name="LAT"/>
<pin name="!OE"/>
<pin name="DOUT" direction="out"/>
<pin name="VBB" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
</symbol>
<symbol name="MIC5821-REV">
<pin name="VCC" direction="pwr"/>
<pin name="DAT" direction="in"/>
<pin name="CLK"/>
<pin name="LAT"/>
<pin name="!OE"/>
<pin name="DOUT" direction="out"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
</symbol>
<symbol name="JACK-PLUG">
<pin name="PIN" direction="pas"/>
<pin name="SWITCH" direction="pas"/>
<pin name="OUTER" direction="pas"/>
</symbol>
<symbol name="MXC6202">
<pin name="VDD" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="SCL" function="clk"/>
<pin name="SDA"/>
<pin name="COM" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DS620">
<pin name="VDD" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" function="clk"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="PO" direction="out"/>
</symbol>
<symbol name="JACK-PLUG-1">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="RFM12">
<pin name="!INT!/VDI"/>
<pin name="VDD" direction="pwr"/>
<pin name="SDI"/>
<pin name="SCK"/>
<pin name="!SEL"/>
<pin name="SDO"/>
<pin name="!IRQ" direction="out"/>
<pin name="FSK/DATA/FFS"/>
<pin name="DCLK/CFIL/FFIT" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="!RES"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TSL256X">
<pin name="VDD" direction="pwr"/>
<pin name="ADDR" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in" function="clk"/>
<pin name="INT" direction="out"/>
</symbol>
<symbol name="3V6">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="PIC18(L)F2XK22">
<pin name="VSS1" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="MCLR,VPP,RE3" direction="in"/>
<pin name="RC3,AN15"/>
<pin name="RA6,OSC2,CLKOUT" direction="out"/>
<pin name="RB0,INT0"/>
<pin name="RB1,INT1,AN10"/>
<pin name="RB2,INT2,AN8"/>
<pin name="RB3,AN9,CCP2"/>
<pin name="RB4,AN11"/>
<pin name="RB5,CCP3,PGM"/>
<pin name="RB6,TX2,PGC"/>
<pin name="RB7,RX2,PGD"/>
<pin name="RC0,T1CKI"/>
<pin name="RC1,CCP2,SOSCI"/>
<pin name="RC2,CCP1,T5CKI"/>
<pin name="RC4,AN16"/>
<pin name="RC5,AN17"/>
<pin name="RC6,AN18,TX1"/>
<pin name="RC7,AN19,RX1"/>
<pin name="RA0,AN0"/>
<pin name="RA1,AN1"/>
<pin name="RA2,AN2,VREF-"/>
<pin name="RA3,AN3,VREF+"/>
<pin name="RA4,T0CKI,C1OUT"/>
<pin name="RA5,AN4,HLVDIN,C2OUT"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA7,OSC1,CLKIN" direction="in"/>
</symbol>
<symbol name="CAT6219">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="BYP/ADJ" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PIC18(L)F4XK22">
<pin name="VSS1" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="MCLR,VPP,RE3" direction="in"/>
<pin name="RC3,AN15"/>
<pin name="RA6,OSC2,CLKOUT" direction="out"/>
<pin name="RB0,INT0,AN12"/>
<pin name="RB1,INT1,AN10"/>
<pin name="RB2,INT2,AN8"/>
<pin name="RB3,AN9,CCP2"/>
<pin name="RB4,AN11"/>
<pin name="RB5,AN13,CCP3,PGM"/>
<pin name="RB6,PGC"/>
<pin name="RB7,PGD"/>
<pin name="RC0,T1CKI"/>
<pin name="RC1,CCP2,SOSCI"/>
<pin name="RC2,CCP1,T5CKI"/>
<pin name="RC4,AN16"/>
<pin name="RC5,AN17"/>
<pin name="RC6,AN18,TX1"/>
<pin name="RC7,AN19,RX1"/>
<pin name="RA0,AN0"/>
<pin name="RA1,AN1"/>
<pin name="RA2,AN2,VREF-"/>
<pin name="RA3,AN3,VREF+"/>
<pin name="RA4,T0CKI,C1OUT"/>
<pin name="RA5,AN4,HLVDIN,C2OUT"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RA7,OSC1,CLKIN" direction="in"/>
<pin name="RD0,AN20,SCK2"/>
<pin name="RD1,AN21,SDA2"/>
<pin name="RD2,AN22"/>
<pin name="RD3,AN23,!SS2"/>
<pin name="RD4,AN24,SDO2"/>
<pin name="RD5,AN25"/>
<pin name="RD6,AN26,TX2"/>
<pin name="RD7,AN27,RX2"/>
<pin name="RE0,AN5"/>
<pin name="RE2,AN7"/>
<pin name="RE1,AN6"/>
<pin name="VDD2" direction="pwr"/>
</symbol>
<symbol name="MINI-USB">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="DS1337">
<pin name="X1"/>
<pin name="X2"/>
<pin name="!INTA"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SQW/!INTB!"/>
<pin name="VCC"/>
</symbol>
<symbol name="DS1337C">
<pin name="!INTA"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SQW/!INTB!"/>
<pin name="VCC"/>
</symbol>
<symbol name="BATTERY-1V2">
<pin name="+VE1" direction="pas"/>
<pin name="-VE1" direction="pas"/>
<pin name="-VE2" direction="pas"/>
<pin name="+VE2" direction="pas"/>
</symbol>
<symbol name="L-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PIC12(L)F1822">
<pin name="VSS" direction="pwr"/>
<pin name="RA0,AN0,ICSPDAT"/>
<pin name="RA1,AN1,ICSPCLK"/>
<pin name="RA2,AN2"/>
<pin name="RA3,!MCLR,VPP" direction="in"/>
<pin name="RA4,AN3"/>
<pin name="RA5"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="N-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="SW_4POS">
<pin name="C" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="1" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD1X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD-ICD">
<pin name="VPP" direction="pas" function="dot"/>
<pin name="+V" direction="pwr" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="PGD" direction="pas" function="dot"/>
<pin name="PGC" direction="pas" function="dot"/>
</symbol>
<symbol name="USB">
<pin name="VBUS" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="TSOP-IR-RECEIVER">
<pin name="VO" direction="oc"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SW-DPDT-LED">
<pin name="2"/>
<pin name="5"/>
<pin name="1"/>
<pin name="3"/>
<pin name="4"/>
<pin name="6"/>
<pin name="LED+"/>
<pin name="LED-"/>
</symbol>
<symbol name="CURRENT-SOURCE">
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="R" direction="pas"/>
</symbol>
<symbol name="TPS6734">
<pin name="EN"/>
<pin name="REF"/>
<pin name="SS"/>
<pin name="COMP"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="FB"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="FT230XS">
<description>FT230XS (SSOP-16 version)

http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf</description>
<pin name="3V3OUT"/>
<pin name="USB-"/>
<pin name="USB+"/>
<pin name="!RESET"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="CBUS3"/>
<pin name="CBUS2"/>
<pin name="CBUS1"/>
<pin name="CBUS0"/>
<pin name="!CTS"/>
<pin name="!RTS"/>
<pin name="RXD"/>
<pin name="TXD"/>
<pin name="VCC"/>
<pin name="VCCIO"/>
</symbol>
<symbol name="FT230XQ">
<description>FTDI FT230XQ (QFN-16 version)

http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf</description>
<pin name="3V3OUT"/>
<pin name="USB-"/>
<pin name="USB+"/>
<pin name="!RESET"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="CBUS3"/>
<pin name="CBUS2"/>
<pin name="CBUS1"/>
<pin name="CBUS0"/>
<pin name="!CTS"/>
<pin name="!RTS"/>
<pin name="RXD"/>
<pin name="TXD"/>
<pin name="VCC"/>
<pin name="VCCIO"/>
<pin name="GND_PAD"/>
</symbol>
<symbol name="PINHD1X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="P-MOSFET">
<pin name="D1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="G1" direction="pas"/>
</symbol>
<symbol name="PINHD1X6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="TLC5951">
<pin name="GSSOUT"/>
<pin name="DCSOUT"/>
<pin name="GSSIN"/>
<pin name="GSSCK"/>
<pin name="GSLAT"/>
<pin name="DCSIN"/>
<pin name="DCSCK"/>
<pin name="XBLNK"/>
<pin name="GSCKR"/>
<pin name="GSCKG"/>
<pin name="GSCKB"/>
<pin name="IREF"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="8RED">
<pin name="R1" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="R4" direction="in"/>
<pin name="R5" direction="in"/>
<pin name="R6" direction="in"/>
<pin name="R7" direction="in"/>
<pin name="R0" direction="in"/>
</symbol>
<symbol name="8GREEN">
<pin name="G1" direction="in"/>
<pin name="G2" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="G4" direction="in"/>
<pin name="G5" direction="in"/>
<pin name="G6" direction="in"/>
<pin name="G7" direction="in"/>
<pin name="G0" direction="in"/>
</symbol>
<symbol name="8BLUE">
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B0" direction="in"/>
</symbol>
<symbol name="LDO-4PIN">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT@TAB" direction="pas"/>
<pin name="OUT@2"/>
</symbol>
<symbol name="COAX">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="14-SEGMENT">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="J" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="L" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="AN2" direction="pas"/>
<pin name="AN1" direction="pas"/>
<pin name="DP1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MIC5821" prefix="IC">
<description>8-Bit Serial-Input Latched Drivers</description>
<gates>
<gate name="G$1" symbol="MIC5821"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!OE" pad="7"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DAT" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LAT" pad="6"/>
<connect gate="G$1" pin="O0" pad="16"/>
<connect gate="G$1" pin="O1" pad="15"/>
<connect gate="G$1" pin="O2" pad="14"/>
<connect gate="G$1" pin="O3" pad="13"/>
<connect gate="G$1" pin="O4" pad="12"/>
<connect gate="G$1" pin="O5" pad="11"/>
<connect gate="G$1" pin="O6" pad="10"/>
<connect gate="G$1" pin="O7" pad="9"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VEE" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5891">
<description>8-Bit Serial-Input Latched Source Driver</description>
<gates>
<gate name="G$1" symbol="MIC5891"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DAT" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="16"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LAT" pad="4"/>
<connect gate="G$1" pin="O0" pad="5"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="7"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="O4" pad="9"/>
<connect gate="G$1" pin="O5" pad="10"/>
<connect gate="G$1" pin="O6" pad="11"/>
<connect gate="G$1" pin="O7" pad="12"/>
<connect gate="G$1" pin="VBB" pad="13"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NFM-12881BG-11">
<description>Futurlec 8x8 LED Matrix</description>
<gates>
<gate name="G$1" symbol="8X8MATRIX"/>
</gates>
<devices>
<device name="" package="NFM-12881BG-11">
<connects>
<connect gate="G$1" pin="1" pad="9"/>
<connect gate="G$1" pin="1'" pad="13"/>
<connect gate="G$1" pin="2" pad="14"/>
<connect gate="G$1" pin="2'" pad="3"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="3'" pad="4"/>
<connect gate="G$1" pin="4" pad="12"/>
<connect gate="G$1" pin="4'" pad="10"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="5'" pad="6"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="6'" pad="11"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="7'" pad="15"/>
<connect gate="G$1" pin="8" pad="5"/>
<connect gate="G$1" pin="8'" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5891-REV">
<description>8-Bit Serial-Input Latched Source Driver (output pin order reversed in symbol, for easier use on schematics)</description>
<gates>
<gate name="G$1" symbol="MIC5891-REV"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DAT" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="16"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LAT" pad="4"/>
<connect gate="G$1" pin="O0" pad="5"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="7"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="O4" pad="9"/>
<connect gate="G$1" pin="O5" pad="10"/>
<connect gate="G$1" pin="O6" pad="11"/>
<connect gate="G$1" pin="O7" pad="12"/>
<connect gate="G$1" pin="VBB" pad="13"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5821-REV">
<description>8-Bit Serial-Input Latched Drivers (output pin order reversed for schematics)</description>
<gates>
<gate name="G$1" symbol="MIC5821-REV"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!OE" pad="7"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DAT" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LAT" pad="6"/>
<connect gate="G$1" pin="O0" pad="16"/>
<connect gate="G$1" pin="O1" pad="15"/>
<connect gate="G$1" pin="O2" pad="14"/>
<connect gate="G$1" pin="O3" pad="13"/>
<connect gate="G$1" pin="O4" pad="12"/>
<connect gate="G$1" pin="O5" pad="11"/>
<connect gate="G$1" pin="O6" pad="10"/>
<connect gate="G$1" pin="O7" pad="9"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VEE" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-JACK" prefix="JACK">
<gates>
<gate name="G$1" symbol="JACK-PLUG"/>
</gates>
<devices>
<device name="" package="DC-SOCKET">
<connects>
<connect gate="G$1" pin="OUTER" pad="P$3"/>
<connect gate="G$1" pin="PIN" pad="P$1"/>
<connect gate="G$1" pin="SWITCH" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXC6202">
<description>MXC6202

Ultra Low Cost, ±2.0 g Dual Axis Accelerometer With I2C Interface</description>
<gates>
<gate name="G$1" symbol="MXC6202"/>
</gates>
<devices>
<device name="" package="LCC8">
<connects>
<connect gate="G$1" pin="COM" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS620" uservalue="yes">
<description>Maxim DS620 Low-Voltage, ±0.5°C Accuracy
Digital Thermometer and Thermostat</description>
<gates>
<gate name="G$1" symbol="DS620"/>
</gates>
<devices>
<device name="" package="UMAX8-THERMAL">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PO" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK-PLUG" prefix="J" uservalue="yes">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;br&gt;
Power Jack, DC, Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Drawing: &lt;b&gt;84N1161.pdf / 84N1162.pdf&lt;/b&gt;&lt;br&gt;
Manufacturer: &lt;b&gt;SPC Technology (www.spctechnology.com)&lt;/b&gt;&lt;br&gt;
Type: &lt;b&gt;SPC4077 / SPC 4078&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="JACK-PLUG-1"/>
</gates>
<devices>
<device name="" package="SPC4077-BIG-HOLES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM12">
<gates>
<gate name="G$1" symbol="RFM12"/>
</gates>
<devices>
<device name="" package="RFM12-PIN">
<connects>
<connect gate="G$1" pin="!INT!/VDI" pad="1"/>
<connect gate="G$1" pin="!IRQ" pad="7"/>
<connect gate="G$1" pin="!RES" pad="11"/>
<connect gate="G$1" pin="!SEL" pad="5"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="DCLK/CFIL/FFIT" pad="9"/>
<connect gate="G$1" pin="FSK/DATA/FFS" pad="8"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="6"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSL256*" prefix="U">
<description>Texas Instruments

TSL2560 (SMBus), TSL2561 (I2C) Light-to-digital converter</description>
<gates>
<gate name="G$1" symbol="TSL256X"/>
</gates>
<devices>
<device name="" package="TMB-6">
<connects>
<connect gate="G$1" pin="ADDR" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="INT" pad="5"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="0">
<attribute name="INTERFACE" value="SMBus"/>
</technology>
<technology name="1">
<attribute name="INTERFACE" value="I2C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATT-CR123A">
<description>CR123A (2/3rd AA) battery holder

Manufacturer: Keystone
Mouser part: 534-1019</description>
<gates>
<gate name="G$1" symbol="3V6"/>
</gates>
<devices>
<device name="" package="KEYSTONE-2/3A">
<connects>
<connect gate="G$1" pin="+" pad="+VE"/>
<connect gate="G$1" pin="-" pad="-VE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2XK22">
<description>Microchip PIC18F2xK22 with nanoWatt technology</description>
<gates>
<gate name="G$1" symbol="PIC18(L)F2XK22"/>
</gates>
<devices>
<device name="-SO" package="SOIC28">
<connects>
<connect gate="G$1" pin="MCLR,VPP,RE3" pad="1"/>
<connect gate="G$1" pin="RA0,AN0" pad="2"/>
<connect gate="G$1" pin="RA1,AN1" pad="3"/>
<connect gate="G$1" pin="RA2,AN2,VREF-" pad="4"/>
<connect gate="G$1" pin="RA3,AN3,VREF+" pad="5"/>
<connect gate="G$1" pin="RA4,T0CKI,C1OUT" pad="6"/>
<connect gate="G$1" pin="RA5,AN4,HLVDIN,C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6,OSC2,CLKOUT" pad="10"/>
<connect gate="G$1" pin="RA7,OSC1,CLKIN" pad="9"/>
<connect gate="G$1" pin="RB0,INT0" pad="21"/>
<connect gate="G$1" pin="RB1,INT1,AN10" pad="22"/>
<connect gate="G$1" pin="RB2,INT2,AN8" pad="23"/>
<connect gate="G$1" pin="RB3,AN9,CCP2" pad="24"/>
<connect gate="G$1" pin="RB4,AN11" pad="25"/>
<connect gate="G$1" pin="RB5,CCP3,PGM" pad="26"/>
<connect gate="G$1" pin="RB6,TX2,PGC" pad="27"/>
<connect gate="G$1" pin="RB7,RX2,PGD" pad="28"/>
<connect gate="G$1" pin="RC0,T1CKI" pad="11"/>
<connect gate="G$1" pin="RC1,CCP2,SOSCI" pad="12"/>
<connect gate="G$1" pin="RC2,CCP1,T5CKI" pad="13"/>
<connect gate="G$1" pin="RC3,AN15" pad="14"/>
<connect gate="G$1" pin="RC4,AN16" pad="15"/>
<connect gate="G$1" pin="RC5,AN17" pad="16"/>
<connect gate="G$1" pin="RC6,AN18,TX1" pad="17"/>
<connect gate="G$1" pin="RC7,AN19,RX1" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="MCLR,VPP,RE3" pad="1"/>
<connect gate="G$1" pin="RA0,AN0" pad="2"/>
<connect gate="G$1" pin="RA1,AN1" pad="3"/>
<connect gate="G$1" pin="RA2,AN2,VREF-" pad="4"/>
<connect gate="G$1" pin="RA3,AN3,VREF+" pad="5"/>
<connect gate="G$1" pin="RA4,T0CKI,C1OUT" pad="6"/>
<connect gate="G$1" pin="RA5,AN4,HLVDIN,C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6,OSC2,CLKOUT" pad="10"/>
<connect gate="G$1" pin="RA7,OSC1,CLKIN" pad="9"/>
<connect gate="G$1" pin="RB0,INT0" pad="21"/>
<connect gate="G$1" pin="RB1,INT1,AN10" pad="22"/>
<connect gate="G$1" pin="RB2,INT2,AN8" pad="23"/>
<connect gate="G$1" pin="RB3,AN9,CCP2" pad="24"/>
<connect gate="G$1" pin="RB4,AN11" pad="25"/>
<connect gate="G$1" pin="RB5,CCP3,PGM" pad="26"/>
<connect gate="G$1" pin="RB6,TX2,PGC" pad="27"/>
<connect gate="G$1" pin="RB7,RX2,PGD" pad="28"/>
<connect gate="G$1" pin="RC0,T1CKI" pad="11"/>
<connect gate="G$1" pin="RC1,CCP2,SOSCI" pad="12"/>
<connect gate="G$1" pin="RC2,CCP1,T5CKI" pad="13"/>
<connect gate="G$1" pin="RC3,AN15" pad="14"/>
<connect gate="G$1" pin="RC4,AN16" pad="15"/>
<connect gate="G$1" pin="RC5,AN17" pad="16"/>
<connect gate="G$1" pin="RC6,AN18,TX1" pad="17"/>
<connect gate="G$1" pin="RC7,AN19,RX1" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT6219">
<description>ON Semiconductor 500mA CMOS LDO Regulator</description>
<gates>
<gate name="G$1" symbol="CAT6219"/>
</gates>
<devices>
<device name="-TD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BYP/ADJ" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4XK22">
<description>40/44-Pin, Low-Power, High-Performance
Microcontrollers with nanoWatt XLP Technology</description>
<gates>
<gate name="G$1" symbol="PIC18(L)F4XK22"/>
</gates>
<devices>
<device name="-TQFP44" package="TQFP44">
<connects>
<connect gate="G$1" pin="MCLR,VPP,RE3" pad="18"/>
<connect gate="G$1" pin="RA0,AN0" pad="19"/>
<connect gate="G$1" pin="RA1,AN1" pad="20"/>
<connect gate="G$1" pin="RA2,AN2,VREF-" pad="21"/>
<connect gate="G$1" pin="RA3,AN3,VREF+" pad="22"/>
<connect gate="G$1" pin="RA4,T0CKI,C1OUT" pad="23"/>
<connect gate="G$1" pin="RA5,AN4,HLVDIN,C2OUT" pad="24"/>
<connect gate="G$1" pin="RA6,OSC2,CLKOUT" pad="31"/>
<connect gate="G$1" pin="RA7,OSC1,CLKIN" pad="30"/>
<connect gate="G$1" pin="RB0,INT0,AN12" pad="8"/>
<connect gate="G$1" pin="RB1,INT1,AN10" pad="9"/>
<connect gate="G$1" pin="RB2,INT2,AN8" pad="10"/>
<connect gate="G$1" pin="RB3,AN9,CCP2" pad="11"/>
<connect gate="G$1" pin="RB4,AN11" pad="14"/>
<connect gate="G$1" pin="RB5,AN13,CCP3,PGM" pad="15"/>
<connect gate="G$1" pin="RB6,PGC" pad="16"/>
<connect gate="G$1" pin="RB7,PGD" pad="17"/>
<connect gate="G$1" pin="RC0,T1CKI" pad="32"/>
<connect gate="G$1" pin="RC1,CCP2,SOSCI" pad="35"/>
<connect gate="G$1" pin="RC2,CCP1,T5CKI" pad="36"/>
<connect gate="G$1" pin="RC3,AN15" pad="37"/>
<connect gate="G$1" pin="RC4,AN16" pad="42"/>
<connect gate="G$1" pin="RC5,AN17" pad="43"/>
<connect gate="G$1" pin="RC6,AN18,TX1" pad="44"/>
<connect gate="G$1" pin="RC7,AN19,RX1" pad="1"/>
<connect gate="G$1" pin="RD0,AN20,SCK2" pad="38"/>
<connect gate="G$1" pin="RD1,AN21,SDA2" pad="39"/>
<connect gate="G$1" pin="RD2,AN22" pad="40"/>
<connect gate="G$1" pin="RD3,AN23,!SS2" pad="41"/>
<connect gate="G$1" pin="RD4,AN24,SDO2" pad="2"/>
<connect gate="G$1" pin="RD5,AN25" pad="3"/>
<connect gate="G$1" pin="RD6,AN26,TX2" pad="4"/>
<connect gate="G$1" pin="RD7,AN27,RX2" pad="5"/>
<connect gate="G$1" pin="RE0,AN5" pad="25"/>
<connect gate="G$1" pin="RE1,AN6" pad="26"/>
<connect gate="G$1" pin="RE2,AN7" pad="27"/>
<connect gate="G$1" pin="VDD1" pad="7"/>
<connect gate="G$1" pin="VDD2" pad="28"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI-USB">
<description>Mini USB connector (Kyocera part: 24 5141 005 000 863+)

Farnell order code: 1558179</description>
<gates>
<gate name="G$1" symbol="MINI-USB"/>
</gates>
<devices>
<device name="" package="MINI-USB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1337" prefix="S+">
<description>DS1337 I2C serial real-time clock

Low-power clock/calendar with two programmable time-of-day alarms and a programmable square-wave output.

http://pdfserv.maxim-ic.com/en/ds/DS1337-DS1337C.pdf</description>
<gates>
<gate name="G$1" symbol="DS1337"/>
</gates>
<devices>
<device name="S+" package="SO8">
<connects>
<connect gate="G$1" pin="!INTA" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/!INTB!" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="+" package="DIL8">
<connects>
<connect gate="G$1" pin="!INTA" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/!INTB!" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATT-SNAP-CR123A">
<description>CR123A holder made using two Keystone 92 battery clips.</description>
<gates>
<gate name="G$1" symbol="3V6"/>
</gates>
<devices>
<device name="" package="KEYSTONE-CLIP-2/3A">
<connects>
<connect gate="G$1" pin="+" pad="+VE1"/>
<connect gate="G$1" pin="-" pad="-VE1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATT-SNAP-2/3AAA">
<description>A 2/3rd AAA holder made using two Keystone 82 battery clips.</description>
<gates>
<gate name="G$1" symbol="BATTERY-1V2"/>
</gates>
<devices>
<device name="" package="KEYSTONE-CLIP-2/3AAA">
<connects>
<connect gate="G$1" pin="+VE1" pad="+VE1"/>
<connect gate="G$1" pin="+VE2" pad="+VE2"/>
<connect gate="G$1" pin="-VE1" pad="-VE1"/>
<connect gate="G$1" pin="-VE2" pad="-VE2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR-L1210">
<description>Inductor, L1210 SMD case</description>
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="" package="L1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC12F1822">
<gates>
<gate name="G$1" symbol="PIC12(L)F1822"/>
</gates>
<devices>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="RA0,AN0,ICSPDAT" pad="7"/>
<connect gate="G$1" pin="RA1,AN1,ICSPCLK" pad="6"/>
<connect gate="G$1" pin="RA2,AN2" pad="5"/>
<connect gate="G$1" pin="RA3,!MCLR,VPP" pad="4"/>
<connect gate="G$1" pin="RA4,AN3" pad="3"/>
<connect gate="G$1" pin="RA5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMV22EN">
<description>PMV22EN (NXP Semiconductor)

30 V, 5.2 A N-channel Trench MOSFET</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCRM3A-10R">
<description>Multicomp MCRM3A-10R 10 position rotary switch, SMD.</description>
<gates>
<gate name="G$1" symbol="SW_4POS"/>
</gates>
<devices>
<device name="" package="ROTARY-MCRM3A-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD1X5">
<gates>
<gate name="G$1" symbol="PINHD1X5"/>
</gates>
<devices>
<device name="SQUARE" package="PINHD1X05-SQUARE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="PINHD1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN-ICD" prefix="ICD">
<gates>
<gate name="G$1" symbol="PINHD-ICD"/>
</gates>
<devices>
<device name="" package="PINHD-ICD">
<connects>
<connect gate="G$1" pin="+V" pad="+V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PGC" pad="PGC"/>
<connect gate="G$1" pin="PGD" pad="PGD"/>
<connect gate="G$1" pin="VPP" pad="VPP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-B">
<description>USB B connector</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="" package="TYCO-USB-B-RA">
<connects>
<connect gate="G$1" pin="D+" pad="P$3"/>
<connect gate="G$1" pin="D-" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="VBUS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSOP62XX" uservalue="yes">
<description>Vishay IR Receivers for remote control systems

30 kHz TSOP6230
33 kHz TSOP6233
36 kHz TSOP6236
36.7 kHz TSOP6237
38 kHz TSOP6238
40 kHz TSOP6240
56 kHz TSOP6256</description>
<gates>
<gate name="G$1" symbol="TSOP-IR-RECEIVER"/>
</gates>
<devices>
<device name="" package="VISHAY-TSOP62XX">
<connects>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="VO" pad="P$4"/>
<connect gate="G$1" pin="VS" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WURTH-744711010">
<description>WUERTH ELEKTRONIK - 744711010 - INDUCTOR, ROD CORE 10.0UH 10.0 A</description>
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="" package="WURTH-744711010">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD1X2">
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="PINHD1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQ" package="PINHD1X02-SQUARE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJS-PB61302">
<description>Illuminated DPDT switch, made by RJS Electronics.

Previously Rapid 78-2265</description>
<gates>
<gate name="G$1" symbol="SW-DPDT-LED"/>
</gates>
<devices>
<device name="" package="RJS-SW-ILLUMINATED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="LED+" pad="LED+"/>
<connect gate="G$1" pin="LED-" pad="LED-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM*34">
<description>ST Microelectronics LM134-LM234-LM334

Datasheet: http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00000458.pdf

Pinout is different to Linear model.</description>
<gates>
<gate name="G$1" symbol="CURRENT-SOURCE"/>
</gates>
<devices>
<device name="D" package="SO8">
<connects>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6734">
<gates>
<gate name="G$1" symbol="TPS6734"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="COMP" pad="4"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="2"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO8">
<connects>
<connect gate="G$1" pin="COMP" pad="4"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="2"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT230XQ">
<description>FTDI FT230XQ - USB to basic UART

http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf</description>
<gates>
<gate name="G$1" symbol="FT230XQ"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="G$1" pin="!CTS" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="9"/>
<connect gate="G$1" pin="!RTS" pad="16"/>
<connect gate="G$1" pin="3V3OUT" pad="8"/>
<connect gate="G$1" pin="CBUS0" pad="12"/>
<connect gate="G$1" pin="CBUS1" pad="11"/>
<connect gate="G$1" pin="CBUS2" pad="5"/>
<connect gate="G$1" pin="CBUS3" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="13"/>
<connect gate="G$1" pin="GND_PAD" pad="EXP"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="TXD" pad="15"/>
<connect gate="G$1" pin="USB+" pad="6"/>
<connect gate="G$1" pin="USB-" pad="7"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT230XS">
<description>FT230XS - USB to basic UART convertor

http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf</description>
<gates>
<gate name="G$1" symbol="FT230XS"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="!CTS" pad="6"/>
<connect gate="G$1" pin="!RESET" pad="11"/>
<connect gate="G$1" pin="!RTS" pad="2"/>
<connect gate="G$1" pin="3V3OUT" pad="10"/>
<connect gate="G$1" pin="CBUS0" pad="15"/>
<connect gate="G$1" pin="CBUS1" pad="14"/>
<connect gate="G$1" pin="CBUS2" pad="7"/>
<connect gate="G$1" pin="CBUS3" pad="16"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND1" pad="13"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USB+" pad="8"/>
<connect gate="G$1" pin="USB-" pad="9"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VCCIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD1X4">
<gates>
<gate name="G$1" symbol="PINHD1X4"/>
</gates>
<devices>
<device name="" package="PINHD1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQUARE" package="PINHD1X04-SQUARE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P-MOSFET">
<description>Generic P MOSFET device</description>
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="-SOT23-GSD" package="SOT23">
<connects>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="G1" pad="1"/>
<connect gate="G$1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD1X6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD1X6">
<gates>
<gate name="G$1" symbol="PINHD1X6"/>
</gates>
<devices>
<device name="" package="PINHD1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQUARE" package="PINHD1X06-SQUARE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5951">
<description>&lt;p&gt;&lt;b&gt;TLC5951&lt;/b&gt;
&lt;p&gt;24-Channel, 12-Bit PWM LED Driver with 7-Bit Dot Correction
and 3-Group, 8-Bit Global Brightness Control
&lt;p&gt;This part uses the "correct" footprint from texas.lbr</description>
<gates>
<gate name="BLUE" symbol="8BLUE"/>
<gate name="GREEN" symbol="8GREEN"/>
<gate name="RED" symbol="8RED"/>
<gate name="CHIP" symbol="TLC5951"/>
</gates>
<devices>
<device name="" package="HTSSOP38DAP">
<connects>
<connect gate="BLUE" pin="B0" pad="9"/>
<connect gate="BLUE" pin="B1" pad="12"/>
<connect gate="BLUE" pin="B2" pad="15"/>
<connect gate="BLUE" pin="B3" pad="18"/>
<connect gate="BLUE" pin="B4" pad="21"/>
<connect gate="BLUE" pin="B5" pad="24"/>
<connect gate="BLUE" pin="B6" pad="27"/>
<connect gate="BLUE" pin="B7" pad="30"/>
<connect gate="CHIP" pin="DCSCK" pad="37"/>
<connect gate="CHIP" pin="DCSIN" pad="38"/>
<connect gate="CHIP" pin="DCSOUT" pad="20"/>
<connect gate="CHIP" pin="GND" pad="33"/>
<connect gate="CHIP" pin="GSCKB" pad="6"/>
<connect gate="CHIP" pin="GSCKG" pad="4"/>
<connect gate="CHIP" pin="GSCKR" pad="5"/>
<connect gate="CHIP" pin="GSLAT" pad="3"/>
<connect gate="CHIP" pin="GSSCK" pad="2"/>
<connect gate="CHIP" pin="GSSIN" pad="1"/>
<connect gate="CHIP" pin="GSSOUT" pad="19"/>
<connect gate="CHIP" pin="IREF" pad="34"/>
<connect gate="CHIP" pin="VCC" pad="35"/>
<connect gate="CHIP" pin="XBLNK" pad="36"/>
<connect gate="GREEN" pin="G0" pad="7"/>
<connect gate="GREEN" pin="G1" pad="10"/>
<connect gate="GREEN" pin="G2" pad="13"/>
<connect gate="GREEN" pin="G3" pad="16"/>
<connect gate="GREEN" pin="G4" pad="23"/>
<connect gate="GREEN" pin="G5" pad="26"/>
<connect gate="GREEN" pin="G6" pad="29"/>
<connect gate="GREEN" pin="G7" pad="32"/>
<connect gate="RED" pin="R0" pad="8"/>
<connect gate="RED" pin="R1" pad="11"/>
<connect gate="RED" pin="R2" pad="14"/>
<connect gate="RED" pin="R3" pad="17"/>
<connect gate="RED" pin="R4" pad="22"/>
<connect gate="RED" pin="R5" pad="25"/>
<connect gate="RED" pin="R6" pad="28"/>
<connect gate="RED" pin="R7" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AP1117" prefix="IC">
<description>&lt;b&gt;500 mA Adjustable Output Positive Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
<gates>
<gate name="G$1" symbol="LDO-4PIN"/>
</gates>
<devices>
<device name="MSTT3" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="2"/>
<connect gate="G$1" pin="OUT@TAB" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COAX-F-PCB">
<gates>
<gate name="G$1" symbol="COAX"/>
</gates>
<devices>
<device name="" package="F-COAX-PCB">
<connects>
<connect gate="G$1" pin="1" pad="SIGNAL"/>
<connect gate="G$1" pin="2" pad="GND$1 GND$2 GND$3 GND$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PDA54-11EWA">
<description>Kingbright PDA54-11EWA

14 segment common anode LED display</description>
<gates>
<gate name="G$1" symbol="14-SEGMENT"/>
</gates>
<devices>
<device name="" package="PDA54-11XX">
<connects>
<connect gate="G$1" pin="A" pad="P$12"/>
<connect gate="G$1" pin="AN1" pad="P$16"/>
<connect gate="G$1" pin="AN2" pad="P$11"/>
<connect gate="G$1" pin="B" pad="P$10"/>
<connect gate="G$1" pin="C" pad="P$9"/>
<connect gate="G$1" pin="D" pad="P$7"/>
<connect gate="G$1" pin="DP1" pad="P$8"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="F" pad="P$18"/>
<connect gate="G$1" pin="G" pad="P$17"/>
<connect gate="G$1" pin="H" pad="P$15"/>
<connect gate="G$1" pin="J" pad="P$14"/>
<connect gate="G$1" pin="K" pad="P$6"/>
<connect gate="G$1" pin="L" pad="P$5"/>
<connect gate="G$1" pin="M" pad="P$4"/>
<connect gate="G$1" pin="N" pad="P$2"/>
<connect gate="G$1" pin="P" pad="P$13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
